Winbox

Starische IP-Adresse f. Ethernet Scnittstelle

Software.Reset:

/system reset-configuration no-defaults=yes

Hardware-Reset: Beim Einschalten „res“-Knopf gedrückt halten, bis „User“-LED blinkt

Interface bridge add name=bridge1

Interface bridge port add bridge=bridge1 interface=ether1

Interface bridge port add bridge=bridge1 interface=ether4

Interface bridge port add bridge=bridge1 interface=ether5

Ip addres add interface=bridge1 address 192.168.2.1/24

Ip addres add interface=ether2 address=10.0.0.6/30

Ip addres add interface=ether3 address=10.0.0.9/30

Ip route print

/ip route add dst-address=192.168.1.0/24 gateway=10.0.0.10

gateway=10.0.0.5

export

/interface bridge

add name=bridge1

/interface bridge port

add bridge=bridge1 interface=ether1

add bridge=bridge1 interface=ether4

add bridge=bridge1 interface=ether5

/ip address

add address=192.168.2.1/24 interface=bridge1 network=192.168.2.0

add address=10.0.0.6/30 interface=ether2 network=10.0.0.4

add address=10.0.0.9/30 interface=ether3 network=10.0.0.8

/ip route

add distance=1 dst-address=10.0.0.0/30 gateway=10.0.0.5

add distance=1 dst-address=192.168.0.0/24 gateway=10.0.0.5

add distance=1 dst-address=192.168.1.0/24 gateway=10.0.0.10